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1 Start with two k' ead knos. Bring working sting 4 ovr th files. Pas t under
working string 1.

2 Pass workingsing 1 under thefiler stings and over working ting 4.

3 Pull o both working stings 1o ighten the knot, while holding the midd stings steady.
Pullight
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This knotis used 1o attach a folded string to the support —
a piece of diftwood, a dowel,rng or anather sting.
1 Fold the string in haif and place it on top of the support where the
koot wil be tied.

2 Fold the loop o sring behind the support, without twisting the
strings, then pull the two long strands through the loop.

3 pull tight.
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This s the most important and most-

often used knot in macramé, and aso 1
the most vrsatie. I this book I

‘always tie left-facing square knots for
consistency, but you can make them
right-facing if you want, as long as

You are consistent within each poject

LEFT-FACING SQUARE KNOT

1 Make a left facing hafsquare knot page 15,

2 Move working sting 4 tothe left passing it overth fiers and under workingsring 1
Move working trng 110 the righ, pasing under the ilers and over sting 4.

3 Tightenthe square knot by puling on the workingstings, whie hokding te midde svings
steady and makingsure thy ae notovelapping.
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DOUBLE HALF HITCH KNOTS
(OR CLOVE HITCH KNOT)
This versatie knot creates a inear row of knots and can be fitsd!
worked in a diagonal,straightor vertical line. This s the

most common macramé knot ater the square knot.

DOUBLE HALF HITCH (LEFT TO RIGHT)

1 Usesting 1 a5 yourguide, hokding i at an ange o horzontaly i
fonfthe s srgs T sra s sonetines caledhe Mg’ (5 o

or ‘st o
2 Usesting 2.5 yourfistworing sig. Pl ing 2 up and ver

sving 1, makingaloop.

3 Pullgety. You have made a hlf ich kot

8 Repeatseps 1-3 withsing 2.

' Position the two ops ext 0 exch ater.Th second o secures:

the kot Dot pul 0o hard when makingtis knot o you il ose”

theloops around the guide.





